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Ordering details for lift control
	Customer      
Date      
	Person in charge      
Dept.      
	Order

     
	Country of destination
 FORMCHECKBOX 
 Germany

 FORMCHECKBOX 
      
	Protective system 
shaft: IP      
MR:    IP      
	 FORMCHECKBOX 
 Ex areas
 FORMCHECKBOX 
 shaft      
 FORMCHECKBOX 
 pulley room      
 FORMCHECKBOX 
 MR (special!)      

	Control
 FORMCHECKBOX 
 MULTiBUS


 FORMCHECKBOX 
 SLC4-20
	Delivery date      
	
	
	
	

	Regulations
 FORMCHECKBOX 
 EN 81-1/-2  FORMCHECKBOX 
 EN 81-20
 FORMCHECKBOX 
 new build.  FORMCHECKBOX 
modernisation
 FORMCHECKBOX 
 without machine room
 FORMCHECKBOX 
      
	Car guide rails
 FORMCHECKBOX 
 guide rails opposite
 FORMCHECKBOX 
 cantilevered car frame
 FORMCHECKBOX 
 slide  FORMCHECKBOX 
 roller guides
     
	Type of control
 FORMCHECKBOX 
 single trip operation
 FORMCHECKBOX 
 call/send operation
 FORMCHECKBOX 
 one-button  FORMCHECKBOX 
 down coll.
 FORMCHECKBOX 
 two-button collective
 FORMCHECKBOX 
 group with  FORMDROPDOWN 
 lifts
	Supply lines
 FORMCHECKBOX 
 power 400V50Hz3P,N,PE (10%
 FORMCHECKBOX 
      
 FORMCHECKBOX 
 light 230V50Hz, N, PE (10%
 FORMCHECKBOX 
      
 FORMCHECKBOX 
 no light supply line
	Travel height
      m

Shaft height
      m

     

	Drive, type       (if known)
rated speed      m/s

motor rating      kW      (HP)      A

     
	Motor protection by
 FORMCHECKBOX 
 thermistors
 FORMCHECKBOX 
 Bi-metal protective relay for the motor
 FORMCHECKBOX 
 no motor protection in the control       
 FORMCHECKBOX 
 special:      
	Note:

MR temperature monitoring is integrated in the control by standard

	UCM detection by control system

 FORMCHECKBOX 
 by blocking magnet      VDC at overspeed governor and safety catch
 FORMCHECKBOX 
 by service brake

 FORMCHECKBOX 
 by a separate emergency brake type      

            V      
     (second contact on overspeed governor? (see safety circuit))
 FORMCHECKBOX 
 safety valve type      

            V  FORMCHECKBOX 
AC  FORMCHECKBOX 
DC
	Monitoring of shaft head / shaft pit

 FORMCHECKBOX 
 monitoring of short shaft head
 FORMCHECKBOX 
 monitoring of short shaft pit

 FORMCHECKBOX 
 crowd load (sliding down protection), blocking magnet at OG or blocking valve:

          V   FORMCHECKBOX 
AC  FORMCHECKBOX 
DC

	Rope lift
 FORMCHECKBOX 
 single speed  FORMCHECKBOX 
 pole-changing  FORMCHECKBOX 
 planetary gear  FORMCHECKBOX 
 gearless, tacho type       (for gearless please specify the data!)
service brake      V     /     A  FORMCHECKBOX 
 service brake control device         FORMCHECKBOX 
 brake lever monitoring   FORMCHECKBOX 
 brake lining monitoring
 FORMCHECKBOX 
 speed controller        FORMCHECKBOX 
 deliver    FORMCHECKBOX 
 control classic   FORMCHECKBOX 
 control with DCP3   FORMCHECKBOX 
 control with DCP4
 FORMCHECKBOX 
 tacho, deliver  FORMCHECKBOX 
 plastic hand wheel, deliver ( free motor shaft end: length       mm: diameter       mm 
 FORMCHECKBOX 
 relevelling   FORMCHECKBOX 
 indicator of level position

 FORMCHECKBOX 
 forced ventilation by  FORMCHECKBOX 
 thermal contact in the motor  FORMCHECKBOX 
 control   ( fan motor      V     
	 FORMCHECKBOX 
 Emerg. brake against overspeed in up direction
type       
voltage       V      
     

	Hydraulic lift
 FORMCHECKBOX 
 direct  FORMCHECKBOX 
 roped-hydraulic
 FORMCHECKBOX 
 direct starting  FORMCHECKBOX 
 star-delta starting 
 FORMCHECKBOX 
 soft start (for motor)       

 FORMCHECKBOX 
 in the control  FORMCHECKBOX 
 on the hydraulic drive unit
 FORMCHECKBOX 
 deliver (brand: RST-ESB incl. reactor)
	 FORMCHECKBOX 
 hydraulic control block type      
 FORMCHECKBOX 
 valve upward
 FORMCHECKBOX 
 valve downward
 FORMCHECKBOX 
 pump delayed off
 FORMCHECKBOX 
 fast up
 FORMCHECKBOX 
 fast down
 FORMCHECKBOX 
 valves delayed off
 FORMCHECKBOX 
 fast up/down
 FORMCHECKBOX 
 starting valve
 FORMCHECKBOX 
 control voltage      V     
 FORMCHECKBOX 
 emergency voltage      V     /     A
	 FORMCHECKBOX 
 oil cooler, type            V     /     A

 FORMCHECKBOX 
 oil heater      V     /     A
 FORMCHECKBOX 
 leakage oil pump
          V     /     A

	Shaft map
	Safety circuit
	Main switch

 FORMCHECKBOX 
 on the ctrl. cabinet
 FORMCHECKBOX 
 deliver separately 

     
	Main fuses

 FORMCHECKBOX 
 by others

 FORMCHECKBOX 
 in the control
     
	Return control
 FORMCHECKBOX 
on cabinet door
 FORMCHECKBOX 
on the machine
     
	 FORMCHECKBOX 
 Fire emerg. control

     level:      
For lift group: one contact

 FORMCHECKBOX 
 separate for every lift

 FORMCHECKBOX 
 common for all lifts

	Entrance side   A  B
	 FORMCHECKBOX 
 230VAC
 FORMCHECKBOX 
 doors 48VAC
	
	
	
	

	     
	level 32  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 main curr. limit switch 3 pole
	
	
	
	

	     
	level 31  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 limit switch t./b. in MR
	
	
	
	

	     
	level 30  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 limit switch top
	 FORMCHECKBOX 
 Firemen control
     
	 FORMCHECKBOX 
 Out-of-service
     W/level
	
	

	     
	level 29  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 limit switch bottom
	
	
	
	Gong1
 FORMCHECKBOX 
 on the car

 FORMCHECKBOX 
 under the car
 FORMCHECKBOX 
 on landing levels
 FORMCHECKBOX 
 deliver

	     
	level 28  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 pipe rupture safety cont.
	 FORMCHECKBOX 
 Overload
     
	 FORMCHECKBOX 
 Full load
     
	 FORMCHECKBOX 
Zero load
     
	

	     
	level 27  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 minimum pressure 
	
	
	
	

	     
	level 26  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 key bridging min. pressure
	 FORMCHECKBOX 
 Attendant control
     
	 FORMCHECKBOX 
 Occupied indicator
     
	 FORMCHECKBOX 
Car priority
     
	

	     
	level 25  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 buffer contact car+counterwt.
	
	
	
	

	     
	level 24  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 slack rope sw. susp. ropes
	 FORMCHECKBOX 
 External priority
For lift groups:
 FORMCHECKBOX 
 works only on lift No      
 FORMCHECKBOX 
 works on the complete group

     
	Direction arrows2
 FORMCHECKBOX 
 in the car
 FORMCHECKBOX 
 on the levels
     W/level
 FORMCHECKBOX 
 Trav. cont. arrows3 on levels

      W/level

     
	Car position indicator

 FORMCHECKBOX 
 individual lamps
 FORMCHECKBOX 
 digital, 
coding      
common cathode
     W/level

     
	Landing position indicator
 FORMCHECKBOX 
 individual lamps
 FORMCHECKBOX 
 digital, 
coding      
common cathode
     W/level

     

	     
	level 23  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 slack rope sw. comp. ropes
	
	
	
	

	     
	level 22  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 SG (safety gear)
	
	
	
	

	     
	level 21  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 OG (overspeed governor)
	
	
	
	

	     
	level 20  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 OG tension weight switch
	
	
	
	

	     
	level 19  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 OG 2nd contact for SG upwards
	
	
	
	

	     
	level 18  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 OG remote tripping 230VAC
	
	
	
	

	     
	level 17  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 OG remote tripping 207VDC
	
	
	
	

	     
	level 16  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 emerg. exit in car roof
	 FORMCHECKBOX 
 Audible alarm
 FORMCHECKBOX 
 on car term. box
 FORMCHECKBOX 
 in the shaft
 FORMCHECKBOX 
 deliver

     
	 FORMCHECKBOX 
 Remote alarm dev.
     type      
 FORMCHECKBOX 
device in the MR
 FORMCHECKBOX 
on the car 
     
	Car ventilator

 FORMCHECKBOX 
 button 
 FORMCHECKBOX 
 switch 
 FORMCHECKBOX 
 travel (coasting)

     
	Remote shutdown

 FORMCHECKBOX 
 for control 
 FORMCHECKBOX 
 control and light
key switch on level      

	     
	level 15  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 pit ladder contact
	
	
	
	

	     
	level 14  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 emerg. stop in the car
	
	
	
	

	     
	level 13  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 2nd emerg. stop on the car
	
	
	
	

	     
	level 12  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	     (in case of 2 entrance sides)
	
	
	
	

	     
	level 11  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	      FORMCHECKBOX 
 deliver
	Emergency light

 FORMCHECKBOX 
 12V   FORMCHECKBOX 
 24V (MULTiBUS only 24V)
	 FORMCHECKBOX 
 Emerg call relay
 FORMCHECKBOX 
 in car term. box

 FORMCHECKBOX 
 in control 

(normally not needed in case of alarm buttons with a 2nd contact)
	Alarm button 

with 2nd contact
 FORMCHECKBOX 
 yes  FORMCHECKBOX 
 no

(yes for all
 STRACK-panels)

	     
	level 10  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 emergency stop in the pit
	
	
	

	     
	level   9  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	      FORMCHECKBOX 
 deliver
	 FORMCHECKBOX 
 separate intercom
 FORMCHECKBOX 
 deliver   FORMCHECKBOX 
 reserve terminals only

 FORMCHECKBOX 
 telephone outlet

 FORMCHECKBOX 
 on the control

 FORMCHECKBOX 
 in the car

 FORMCHECKBOX 
 on the car terminal box

 FORMCHECKBOX 
 porter’s lodge
	
	

	     
	level   8  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 emerg. stop beside MR door
	
	
	

	     
	level   7  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	      FORMCHECKBOX 
 deliver
	
	
	

	     
	level   6  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
 safety light grid
	
	
	

	     
	level   5  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	      FORMCHECKBOX 
 deliver STRACK LTÜ²
	
	 FORMCHECKBOX 
 Speech unit   FORMCHECKBOX 
 Music  FORMCHECKBOX 
 Stereo

 FORMCHECKBOX 
 deliver STRACK Audio module
texts:      

	     
	level   4  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	     car height      mm
	
	

	     
	level   3  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	      FORMCHECKBOX 
 rear wall installation kit
	
	

	     
	level   2  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	      FORMCHECKBOX 
 surface mount kit
	Distances (cable routing)

	     
	level   1  FORMCHECKBOX 


 FORMCHECKBOX 

	     m
	 FORMCHECKBOX 
      
	
	

	
	
	
	 FORMCHECKBOX 
      
	control - machine      m
control - external speed controller      m

control - shaft        m
machine room  FORMCHECKBOX 
 top  FORMCHECKBOX 
 bottom

height of shaft head (HR)      m

depth of shaft pit (SP)      m
	For lift groups

distance control-control      m
     

	 
	indication of heights or distances is imperative!
	
	

	          floor designations 
	
	
	

	continue next page (


1 With gong on top of and under the car these are operated depending on the travel direction, so that gong is sounding which is nearest to the destination.
2 (Direction) arrows in all levels indicated in parallel (normal with single lifts).
3 (Travel continuation) arrow indicating only on that respective level where the lift is approaching to (normal with groups).
	With opposite car entrance

	 FORMCHECKBOX 
 car call button common for both entrance sides
 FORMCHECKBOX 
 car call button separately for each door side
	 FORMCHECKBOX 
 door-open button common for both entrance sides
 FORMCHECKBOX 
 door-open button separately for each door side
	     

	Doors:
 Manufacturer identification      

	 FORMCHECKBOX 
 Light barrier 

 FORMCHECKBOX 
 light curtain  FORMCHECKBOX 
 deliver
 FORMCHECKBOX 
 incl. red-/green illumination
 FORMCHECKBOX 
 lobby monitoring  FORMCHECKBOX 
 deliver
	 FORMCHECKBOX 
 nudging 

 FORMCHECKBOX 
 pre-opening 
      during travel-in
 FORMCHECKBOX 
      
	 FORMCHECKBOX 
 unlocking magnet / motor
          V     /      A

 FORMCHECKBOX 
 mechanical shaft door locks
 FORMCHECKBOX 
 monitoring contacts for

      unlocking magnet de-energized 
	 FORMCHECKBOX 
 button, loading-time
 FORMCHECKBOX 
 button, door-closing
 FORMCHECKBOX 
      
	 FORMCHECKBOX 
 door sluice on the lev.      
 FORMCHECKBOX 
 separating door in the car
 FORMCHECKBOX 
      

	Side A

Side B
	car door

 FORMCHECKBOX 
 auto  FORMCHECKBOX 
 manually
 FORMCHECKBOX 
 auto  FORMCHECKBOX 
 manually
	Landing door

 FORMCHECKBOX 
 auto  FORMCHECKBOX 
 manually
 FORMCHECKBOX 
 auto  FORMCHECKBOX 
 manually
	Motor

     V     A
     V     A
	Motor protection
 FORMCHECKBOX 
 running time
 FORMCHECKBOX 
+circuit breaker
	limit switch
OPEN
CLOSED
	Door operator control, type

 FORMCHECKBOX 
      
 FORMCHECKBOX 
      

	
	
	
	
	
	
 FORMCHECKBOX 
 yes
 FORMCHECKBOX 
 yes

 FORMCHECKBOX 
 yes
 FORMCHECKBOX 
 yes
	

	 FORMCHECKBOX 
 emergency power evacuation
 FORMCHECKBOX 
 emergency voltage by others
 FORMCHECKBOX 
 with signal contact to control
 FORMCHECKBOX 
 without signal contact to control
 FORMCHECKBOX 
 sequential switching, max. 

     lifts simultaneously  FORMDROPDOWN 

 FORMCHECKBOX 
 connection to external   

     evacuation control
 FORMCHECKBOX 
 only STRACK controls 
     (connected via bus) 

     
	Shaft lighting
button  FORMCHECKBOX 
 in the control  FORMCHECKBOX 
 in control cabinet door 
 FORMCHECKBOX 
 button on top of car
 FORMCHECKBOX 
 button in the shaft pit
 FORMCHECKBOX 
 deliver STRACK MULTiLED-SL
 FORMCHECKBOX 
 deliver special type      
 FORMCHECKBOX 
 with group lifts (common shaft):
     common light switching
     
	Shaft information system
 FORMCHECKBOX 
 deliver of Disk, absolute encoder with knobbed belt (standard)

absolute encoder, special type      
 FORMCHECKBOX 
 deliver

	
	
	 FORMCHECKBOX 
 Car terminal box with inspection panel
     as a flexible control handset with 2nd cable      

	
	
	Alarm button 
 FORMCHECKBOX 
 onto car 




 FORMCHECKBOX 
 in the shaft pit
	 FORMCHECKBOX 
 deliver
 FORMCHECKBOX 
 deliver

	
	
	 FORMCHECKBOX 
 Travellg. cable, deliver
 FORMCHECKBOX 
 pluggable
     m, lengths rounded to full 5m

 FORMCHECKBOX 
 halogen-free
	Standard calculation of length:

MR on top: TH+HR+ 
                   distance CS/shaft +10m

MR below: TH+HR+ 
                   distance CS/shaft +10m

	
	
	Shaft wiring
 FORMCHECKBOX 
 not in delivery
 FORMCHECKBOX 
 deliver incl.:
    FORMCHECKBOX 
 cable duct
    FORMCHECKBOX 
 interlock cable
    FORMCHECKBOX 
 limit switch 

         incl. holder
    FORMCHECKBOX 
 OG tension. wgt. 
         switch incl holder
    FORMCHECKBOX 
 bits and pieces

    FORMCHECKBOX 
 halogen-free

     
	Car wiring
 FORMCHECKBOX 
 not in delivery
 FORMCHECKBOX 
 deliver incl.:

    FORMCHECKBOX 
 zone switch set

    FORMCHECKBOX 
 cable duct
    FORMCHECKBOX 
 halogen-free

     
	MR wiring
 FORMCHECKBOX 
 not in delivery
 FORMCHECKBOX 
 deliver incl.:

    FORMCHECKBOX 
 cable duct
    FORMCHECKBOX 
 motor cable
    FORMCHECKBOX 
 with inverter: 

        EMC fitting 
        for the motor,   
        thread size 
        Pg size      
        M size      
    FORMCHECKBOX 
 with inverter: 

        DCP cable set  
        (pluggable) 

    FORMCHECKBOX 
 main supply
             m

    FORMCHECKBOX 
 halogen-free

     

	Control cabinet (B x H x T) / mm
	
	
	

	Wall-mount cabinet STRACK WS04 (standard)
(IP54 mounted on a flat wall, otherwise IP21)
 FORMCHECKBOX 
   700 x 1300 x 280

 FORMCHECKBOX 
 1000 x 1300 x 280

 FORMCHECKBOX 
 1000 x   900 x 280
	Door-hinge side 

 FORMCHECKBOX 
 right  FORMCHECKBOX 
 left
removable door, triangular lock
	
	
	

	
	
	
	
	

	Wall-mount cabinet WS

 FORMCHECKBOX 
   760 x   760 x 210 IP54
 FORMCHECKBOX 
   800 x   800 x 300 IP54
 FORMCHECKBOX 
   800 x 1000 x 300 IP54
 FORMCHECKBOX 
 1000 x   800 x 300 IP54

 FORMCHECKBOX 
 1000 x 1000 x 300 IP54

 FORMCHECKBOX 
 1000 x 1200 x 300 IP54

 FORMCHECKBOX 
 1200 x 1000 x 300 IP54

 FORMCHECKBOX 
       x       x      


     
	Door-hinge side
 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right
 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

double-wing
 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right  FORMCHECKBOX 
 double-wing
 FORMCHECKBOX 
 triangular lock
 FORMCHECKBOX 
 lock with DIN half cylinder
	
	
	

	
	
	
	
	

	
	
	
	
	

	
	
	
	
	

	Floor-mount cabinet SS

(all dimensions incl. 100mm socket)
 FORMCHECKBOX 
   800 x 1700 x 400 IP54

 FORMCHECKBOX 
 1000 x 1700 x 400 IP54

 FORMCHECKBOX 
   800 x 1900 x 400 IP54

 FORMCHECKBOX 
 1000 x 1900 x 400 IP54

 FORMCHECKBOX 
 1200 x 1900 x 400 IP54

 FORMCHECKBOX 
 1200 x 2100 x 500 IP54

 FORMCHECKBOX 
   300 x 1900 x 130 (standard S-MRL, socket
       integrated)

 FORMCHECKBOX 
       x       x      
     
	Door-hinge side

 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

double-wing
 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

double-wing
double-wing
double-wing
 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right

 FORMCHECKBOX 
 left  FORMCHECKBOX 
 right  FORMCHECKBOX 
 double-wing
 FORMCHECKBOX 
 triangular lock 

 FORMCHECKBOX 
 lock with DIN half cylinder
	Connection to LIFTnet monitoring for lifts
 FORMCHECKBOX 
 preparation only 
 FORMCHECKBOX 
 via emergency call device (provided by customer, pay attention to 
     compatible type)
 FORMCHECKBOX 
 Ethernet
LIFTnet server and clients
 FORMCHECKBOX 
 deliver LIFTnet server/clients, number of work stations  FORMDROPDOWN 

 FORMCHECKBOX 
 deliver only the LIFTnet software, No. of work stations   FORMDROPDOWN 

 FORMCHECKBOX 
 bitmap programming of the building ground plans (special) 

     

	Cabinet for machine-room-less rope lift

 FORMCHECKBOX 
   400 x 2050 x 150 (type S-MRL20) 

      FORMCHECKBOX 
   RAL 7035 (light gray) (standard)
      FORMCHECKBOX 
   stainless steel
 FORMCHECKBOX 
   150 x 1900(+base) x 140 (type MRLmini)
      FORMCHECKBOX 
   base       mm (min. 75, standard 95)

            (selectable in 5mm steps) 

      FORMCHECKBOX 
   stainless steel K240

      FORMCHECKBOX 
   mounting plate only, 118 x 1880 x 10


	Door-hinge side

 FORMCHECKBOX 
 left
 FORMCHECKBOX 
 right
removable door, DIN half cylinder

removable cover, DIN half cylinder

     
	Electronic lift attendant

 FORMCHECKBOX 
 integrated in the lift control
 FORMCHECKBOX 
 extern system      
     

	 FORMCHECKBOX 
 lighting in the cabinet, STRACK MULTiLED-HM   FORMCHECKBOX 
 with door switch
 FORMCHECKBOX 
 wall-outlet in the cabinet
	

	Miscellaneous

     


	continue next page (
	
	


	Car operating panel (COP)

 FORMCHECKBOX 
 conventional, no pre-wiring
 FORMCHECKBOX 
 deliver plug system
 FORMCHECKBOX 
 custom made plug system:      
 FORMCHECKBOX 
 deliver STRACK panels
 FORMCHECKBOX 
 panel  FORMCHECKBOX 
 with mounting box
 FORMCHECKBOX 
 panel  FORMCHECKBOX 
 230  FORMCHECKBOX 
 300  FORMCHECKBOX 
 with      
 FORMCHECKBOX 
 desk type panel 
          
 FORMCHECKBOX 
 emerg. call indicator “please talk“ and 

     “connection active“ acc. to EN81-28

 FORMCHECKBOX 
 info field  (lift data, logo, …)

      FORMCHECKBOX 
 illuminated  FORMCHECKBOX 
 not illuminated

 FORMCHECKBOX 
 further info field  with emergency call text

      FORMCHECKBOX 
 illuminated  FORMCHECKBOX 
 not illuminated

 FORMCHECKBOX 
 info fields beside the command buttons

      FORMCHECKBOX 
 illuminated  FORMCHECKBOX 
 not illuminated

 FORMCHECKBOX 
 key switch button as command for the  
     levels:      
 FORMCHECKBOX 
 key switch, function:
          
 FORMCHECKBOX 
 key switch, function:
          
 FORMCHECKBOX 
 oberve the dimensions, draft is enclosed!
 FORMCHECKBOX 
      
	Hall panels (HP)

 FORMCHECKBOX 
 conventional, no pre-wiring

 FORMCHECKBOX 
 deliver plug system
 FORMCHECKBOX 
 custom made plug system:      
 FORMCHECKBOX 
 deliver STRACK panels
 FORMCHECKBOX 
 in door jamb
 FORMCHECKBOX 
 with mounting box
 FORMCHECKBOX 
 in the wall 
 FORMCHECKBOX 
 with mounting box
          
 FORMCHECKBOX 
 coloured engraving, company logo
 FORMCHECKBOX 
 coloured engraving, fire emergency
 FORMCHECKBOX 
 in case of lift group: 

      FORMCHECKBOX 
 one panel at each lift door

      FORMCHECKBOX 
 one panel between the doors

      FORMCHECKBOX 
 special arrangement, draft is enclosed!
 FORMCHECKBOX 
 observe the dimensions, draft is enclosed!
 FORMCHECKBOX 
      
	Separate hall indicator panels

 FORMCHECKBOX 
 conventional, no pre-wiring

 FORMCHECKBOX 
 deliver plug system
 FORMCHECKBOX 
 custom made plug system:      
 FORMCHECKBOX 
 deliver STRACK panels
 FORMCHECKBOX 
 beside door
 FORMCHECKBOX 
 with mounting box

 FORMCHECKBOX 
 above door
 FORMCHECKBOX 
 with mounting box

 FORMCHECKBOX 
 downward inclined ca. 20°
          
 FORMCHECKBOX 
 observe the dimensions, draft is enclosed!
 FORMCHECKBOX 
       
	If panels are to be

supplied:
capacity      kg
      Persons

CE     
manuf. no.     
or modernization no.
     
year      
manufacturer      
     

	
	
	
	Regulations
 FORMCHECKBOX 
 EN 81-70 („persons with handicaps“)

 FORMCHECKBOX 
 EN 81-71 („vandals“)

      FORMCHECKBOX 
 class 0

      FORMCHECKBOX 
 class 1

      FORMCHECKBOX 
 class 2

	Indicate only if not to standard:

[image: image1.wmf]
1. Panel      :
A  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

B  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

2. Panel      :
A  FORMCHECKBOX 
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B  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
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3. Panel      :
A  FORMCHECKBOX 
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max  FORMCHECKBOX 
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B  FORMCHECKBOX 
min  FORMCHECKBOX 
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4. Panel      :
A  FORMCHECKBOX 
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B  FORMCHECKBOX 
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	Indicate only if not to standard:
[image: image2.wmf]
Panel on floor(s)      :
A  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

B  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

for “0“ only one hole in the middle: 

C  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

D  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

E  FORMCHECKBOX 
M3   FORMCHECKBOX 
M4    FORMCHECKBOX 
M5   FORMCHECKBOX 
weld screws
Panel on floor (s)      :
A  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

B  FORMCHECKBOX 
min  FORMCHECKBOX 
max  FORMCHECKBOX 
exactly       mm

for “0“ only one hole in the middle: 

C  FORMCHECKBOX 
min  FORMCHECKBOX 
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	Legend:

	

	Lev
level (landing)

TH
travel height
OG
overspeed governor
KKL
car terminal box (normally on the car roof, incl
inspection switch, 

wall-outlet, etc, pre-wired)

MR
machine room
SG
safety gear
	S-MRL
control cabinet for machine-room-less rope lift

SH
shaft height
SP
shaft pit
HR
shaft head
SS
floor-mount control cabinet
CS
control system
UCM
unintended car movement

WS
wall mount control cabinet


